**LBK Downstream SR530 (Site AG)**

Site Map (Figure 1)

AG1 – site outlet

Temperature, Water Level, and Connectivity Trends

* No equipment installed at the site because does not hold substantial water to sustain fish
* Site disconnects from the mainstem Skagit but the topography is too flat that when mainstem flows recede the site seems to drain completely

7/15/2021

* Boat reconnaissance
* AG1 outlet not very obvious from the mainstem
* Completely dry, likely just overflow from the two channels on either side (Figure 2)

A picture containing tree, outdoor, forest, plant

Description automatically generated

Figure 2. Flat topography throughout site causes complete draining of the site when mainstem flows recede